    /******************************************************************************
     * memory.h
     *
     * Memory reservation and information.
     *
     * Permission is hereby granted, free of charge, to any person obtaining a copy
     * of this software and associated documentation files (the "Software"), to
     * deal in the Software without restriction, including without limitation the
     * rights to use, copy, modify, merge, publish, distribute, sublicense, and/or
     * sell copies of the Software, and to permit persons to whom the Software is
     * furnished to do so, subject to the following conditions:
     *
     * The above copyright notice and this permission notice shall be included in
     * all copies or substantial portions of the Software.
     *
     * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
     * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
     * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
     * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
     * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
     * FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER
     * DEALINGS IN THE SOFTWARE.
     *
     * Copyright (c) 2005, Keir Fraser <keir@xensource.com>
     */

    #ifndef __XEN_PUBLIC_MEMORY_H__
    #define __XEN_PUBLIC_MEMORY_H__

    #include "xen.h"
    #include "physdev.h"

    /*
     * Increase or decrease the specified domain's memory reservation. Returns the
     * number of extents successfully allocated or freed.
     * arg == addr of struct xen_memory_reservation.
     */
    #define XENMEM_increase_reservation 0
    #define XENMEM_decrease_reservation 1
    #define XENMEM_populate_physmap     6

    #if __XEN_INTERFACE_VERSION__ >= 0x00030209
    /*
     * Maximum # bits addressable by the user of the allocated region (e.g., I/O
     * devices often have a 32-bit limitation even in 64-bit systems). If zero
     * then the user has no addressing restriction. This field is not used by
     * XENMEM_decrease_reservation.
     */
    #define XENMEMF_address_bits(x)     (x)
    #define XENMEMF_get_address_bits(x) ((x) & 0xffu)
    /* NUMA node to allocate from. */
    #define XENMEMF_node(x)     (((x) + 1) << 8)
    #define XENMEMF_get_node(x) ((((x) >> 8) - 1) & 0xffu)
    /* Flag to populate physmap with populate-on-demand entries */
    #define XENMEMF_populate_on_demand (1<<16)
    /* Flag to request allocation only from the node specified */
    #define XENMEMF_exact_node_request  (1<<17)
    #define XENMEMF_exact_node(n) (XENMEMF_node(n) | XENMEMF_exact_node_request)
    /* Flag to indicate the node specified is virtual node */
    #define XENMEMF_vnode  (1<<18)
    #endif

    struct xen_memory_reservation {

        /*
         * XENMEM_increase_reservation:
         *   OUT: MFN (*not* GMFN) bases of extents that were allocated
         * XENMEM_decrease_reservation:
         *   IN:  GMFN bases of extents to free
         * XENMEM_populate_physmap:
         *   IN:  GPFN bases of extents to populate with memory
         *   OUT: GMFN bases of extents that were allocated
         *   (NB. This command also updates the mach_to_phys translation table)
         * XENMEM_claim_pages:
         *   IN: must be zero
         */
        XEN_GUEST_HANDLE(xen_pfn_t) extent_start;

        /* Number of extents, and size/alignment of each (2^extent_order pages). */
        xen_ulong_t    nr_extents;
        unsigned int   extent_order;

    #if __XEN_INTERFACE_VERSION__ >= 0x00030209
        /* XENMEMF flags. */
        unsigned int   mem_flags;
    #else
        unsigned int   address_bits;
    #endif

        /*
         * Domain whose reservation is being changed.
         * Unprivileged domains can specify only DOMID_SELF.
         */
        domid_t        domid;
    };
    typedef struct xen_memory_reservation xen_memory_reservation_t;
    DEFINE_XEN_GUEST_HANDLE(xen_memory_reservation_t);

    /*
     * An atomic exchange of memory pages. If return code is zero then
     * @out.extent_list provides GMFNs of the newly-allocated memory.
     * Returns zero on complete success, otherwise a negative error code.
     * On complete success then always @nr_exchanged == @in.nr_extents.
     * On partial success @nr_exchanged indicates how much work was done.
     */
    #define XENMEM_exchange             11
    struct xen_memory_exchange {
        /*
         * [IN] Details of memory extents to be exchanged (GMFN bases).
         * Note that @in.address_bits is ignored and unused.
         */
        struct xen_memory_reservation in;

        /*
         * [IN/OUT] Details of new memory extents.
         * We require that:
         *  1. @in.domid == @out.domid
         *  2. @in.nr_extents  << @in.extent_order ==
         *     @out.nr_extents << @out.extent_order
         *  3. @in.extent_start and @out.extent_start lists must not overlap
         *  4. @out.extent_start lists GPFN bases to be populated
         *  5. @out.extent_start is overwritten with allocated GMFN bases
         */
        struct xen_memory_reservation out;

        /*
         * [OUT] Number of input extents that were successfully exchanged:
         *  1. The first @nr_exchanged input extents were successfully
         *     deallocated.
         *  2. The corresponding first entries in the output extent list correctly
         *     indicate the GMFNs that were successfully exchanged.
         *  3. All other input and output extents are untouched.
         *  4. If not all input exents are exchanged then the return code of this
         *     command will be non-zero.
         *  5. THIS FIELD MUST BE INITIALISED TO ZERO BY THE CALLER!
         */
        xen_ulong_t nr_exchanged;
    };
    typedef struct xen_memory_exchange xen_memory_exchange_t;
    DEFINE_XEN_GUEST_HANDLE(xen_memory_exchange_t);

    /*
     * Returns the maximum machine frame number of mapped RAM in this system.
     * This command always succeeds (it never returns an error code).
     * arg == NULL.
     */
    #define XENMEM_maximum_ram_page     2

    /*
     * Returns the current or maximum memory reservation, in pages, of the
     * specified domain (may be DOMID_SELF). Returns -ve errcode on failure.
     * arg == addr of domid_t.
     */
    #define XENMEM_current_reservation  3
    #define XENMEM_maximum_reservation  4

    /*
     * Returns the maximum GPFN in use by the guest, or -ve errcode on failure.
     */
    #define XENMEM_maximum_gpfn         14

    /*
     * Returns a list of MFN bases of 2MB extents comprising the machine_to_phys
     * mapping table. Architectures which do not have a m2p table do not implement
     * this command.
     * arg == addr of xen_machphys_mfn_list_t.
     */
    #define XENMEM_machphys_mfn_list    5
    struct xen_machphys_mfn_list {
        /*
         * Size of the 'extent_start' array. Fewer entries will be filled if the
         * machphys table is smaller than max_extents * 2MB.
         */
        unsigned int max_extents;

        /*
         * Pointer to buffer to fill with list of extent starts. If there are
         * any large discontiguities in the machine address space, 2MB gaps in
         * the machphys table will be represented by an MFN base of zero.
         */
        XEN_GUEST_HANDLE(xen_pfn_t) extent_start;

        /*
         * Number of extents written to the above array. This will be smaller
         * than 'max_extents' if the machphys table is smaller than max_e * 2MB.
         */
        unsigned int nr_extents;
    };
    typedef struct xen_machphys_mfn_list xen_machphys_mfn_list_t;
    DEFINE_XEN_GUEST_HANDLE(xen_machphys_mfn_list_t);

    /*
     * For a compat caller, this is identical to XENMEM_machphys_mfn_list.
     *
     * For a non compat caller, this functions similarly to
     * XENMEM_machphys_mfn_list, but returns the mfns making up the compatibility
     * m2p table.
     */
    #define XENMEM_machphys_compat_mfn_list     25

    /*
     * Returns the location in virtual address space of the machine_to_phys
     * mapping table. Architectures which do not have a m2p table, or which do not
     * map it by default into guest address space, do not implement this command.
     * arg == addr of xen_machphys_mapping_t.
     */
    #define XENMEM_machphys_mapping     12
    struct xen_machphys_mapping {
        xen_ulong_t v_start, v_end; /* Start and end virtual addresses.   */
        xen_ulong_t max_mfn;        /* Maximum MFN that can be looked up. */
    };
    typedef struct xen_machphys_mapping xen_machphys_mapping_t;
    DEFINE_XEN_GUEST_HANDLE(xen_machphys_mapping_t);

    /* Source mapping space. */
    /* ` enum phys_map_space { */
    #define XENMAPSPACE_shared_info  0 /* shared info page */
    #define XENMAPSPACE_grant_table  1 /* grant table page */
    #define XENMAPSPACE_gmfn         2 /* GMFN */
    #define XENMAPSPACE_gmfn_range   3 /* GMFN range, XENMEM_add_to_physmap only. */
    #define XENMAPSPACE_gmfn_foreign 4 /* GMFN from another dom,
                                        * XENMEM_add_to_physmap_batch only. */
    #define XENMAPSPACE_dev_mmio     5 /* device mmio region
                                          ARM only; the region is mapped in
                                          Stage-2 using the Normal Memory
                                          Inner/Outer Write-Back Cacheable
                                          memory attribute. */
    /* ` } */

    /*
     * Sets the GPFN at which a particular page appears in the specified guest's
     * pseudophysical address space.
     * arg == addr of xen_add_to_physmap_t.
     */
    #define XENMEM_add_to_physmap      7
    struct xen_add_to_physmap {
        /* Which domain to change the mapping for. */
        domid_t domid;

        /* Number of pages to go through for gmfn_range */
        uint16_t    size;

        unsigned int space; /* => enum phys_map_space */

    #define XENMAPIDX_grant_table_status 0x80000000

        /* Index into space being mapped. */
        xen_ulong_t idx;

        /* GPFN in domid where the source mapping page should appear. */
        xen_pfn_t     gpfn;
    };
    typedef struct xen_add_to_physmap xen_add_to_physmap_t;
    DEFINE_XEN_GUEST_HANDLE(xen_add_to_physmap_t);

    /* A batched version of add_to_physmap. */
    #define XENMEM_add_to_physmap_batch 23
    struct xen_add_to_physmap_batch {
        /* IN */
        /* Which domain to change the mapping for. */
        domid_t domid;
        uint16_t space; /* => enum phys_map_space */

        /* Number of pages to go through */
        uint16_t size;

    #if __XEN_INTERFACE_VERSION__ < 0x00040700
        domid_t foreign_domid; /* IFF gmfn_foreign. Should be 0 for other spaces. */
    #else
        union xen_add_to_physmap_batch_extra {
            domid_t foreign_domid; /* gmfn_foreign */
            uint16_t res0;  /* All the other spaces. Should be 0 */
        } u;
    #endif

        /* Indexes into space being mapped. */
        XEN_GUEST_HANDLE(xen_ulong_t) idxs;

        /* GPFN in domid where the source mapping page should appear. */
        XEN_GUEST_HANDLE(xen_pfn_t) gpfns;

        /* OUT */

        /* Per index error code. */
        XEN_GUEST_HANDLE(int) errs;
    };
    typedef struct xen_add_to_physmap_batch xen_add_to_physmap_batch_t;
    DEFINE_XEN_GUEST_HANDLE(xen_add_to_physmap_batch_t);

    #if __XEN_INTERFACE_VERSION__ < 0x00040400
    #define XENMEM_add_to_physmap_range XENMEM_add_to_physmap_batch
    #define xen_add_to_physmap_range xen_add_to_physmap_batch
    typedef struct xen_add_to_physmap_batch xen_add_to_physmap_range_t;
    DEFINE_XEN_GUEST_HANDLE(xen_add_to_physmap_range_t);
    #endif

    /*
     * Unmaps the page appearing at a particular GPFN from the specified guest's
     * pseudophysical address space.
     * arg == addr of xen_remove_from_physmap_t.
     */
    #define XENMEM_remove_from_physmap      15
    struct xen_remove_from_physmap {
        /* Which domain to change the mapping for. */
        domid_t domid;

        /* GPFN of the current mapping of the page. */
        xen_pfn_t     gpfn;
    };
    typedef struct xen_remove_from_physmap xen_remove_from_physmap_t;
    DEFINE_XEN_GUEST_HANDLE(xen_remove_from_physmap_t);

    /*** REMOVED ***/
    /*#define XENMEM_translate_gpfn_list  8*/

    /*
     * Returns the pseudo-physical memory map as it was when the domain
     * was started (specified by XENMEM_set_memory_map).
     * arg == addr of xen_memory_map_t.
     */
    #define XENMEM_memory_map           9
    struct xen_memory_map {
        /*
         * On call the number of entries which can be stored in buffer. On
         * return the number of entries which have been stored in
         * buffer.
         */
        unsigned int nr_entries;

        /*
         * Entries in the buffer are in the same format as returned by the
         * BIOS INT 0x15 EAX=0xE820 call.
         */
        XEN_GUEST_HANDLE(void) buffer;
    };
    typedef struct xen_memory_map xen_memory_map_t;
    DEFINE_XEN_GUEST_HANDLE(xen_memory_map_t);

    /*
     * Returns the real physical memory map. Passes the same structure as
     * XENMEM_memory_map.
     * Specifying buffer as NULL will return the number of entries required
     * to store the complete memory map.
     * arg == addr of xen_memory_map_t.
     */
    #define XENMEM_machine_memory_map   10

    /*
     * Set the pseudo-physical memory map of a domain, as returned by
     * XENMEM_memory_map.
     * arg == addr of xen_foreign_memory_map_t.
     */
    #define XENMEM_set_memory_map       13
    struct xen_foreign_memory_map {
        domid_t domid;
        struct xen_memory_map map;
    };
    typedef struct xen_foreign_memory_map xen_foreign_memory_map_t;
    DEFINE_XEN_GUEST_HANDLE(xen_foreign_memory_map_t);

    #define XENMEM_set_pod_target       16
    #define XENMEM_get_pod_target       17
    struct xen_pod_target {
        /* IN */
        uint64_t target_pages;
        /* OUT */
        uint64_t tot_pages;
        uint64_t pod_cache_pages;
        uint64_t pod_entries;
        /* IN */
        domid_t domid;
    };
    typedef struct xen_pod_target xen_pod_target_t;

    #if defined(__XEN__) || defined(__XEN_TOOLS__)

    #ifndef uint64_aligned_t
    #define uint64_aligned_t uint64_t
    #endif

    /*
     * Get the number of MFNs saved through memory sharing.
     * The call never fails.
     */
    #define XENMEM_get_sharing_freed_pages    18
    #define XENMEM_get_sharing_shared_pages   19

    #define XENMEM_paging_op                    20
    #define XENMEM_paging_op_nominate           0
    #define XENMEM_paging_op_evict              1
    #define XENMEM_paging_op_prep               2

    struct xen_mem_paging_op {
        uint8_t     op;         /* XENMEM_paging_op_* */
        domid_t     domain;

        /* PAGING_PREP IN: buffer to immediately fill page in */
        uint64_aligned_t    buffer;
        /* Other OPs */
        uint64_aligned_t    gfn;           /* IN:  gfn of page being operated on */
    };
    typedef struct xen_mem_paging_op xen_mem_paging_op_t;
    DEFINE_XEN_GUEST_HANDLE(xen_mem_paging_op_t);

    #define XENMEM_access_op                    21
    #define XENMEM_access_op_set_access         0
    #define XENMEM_access_op_get_access         1
    /*
     * XENMEM_access_op_enable_emulate and XENMEM_access_op_disable_emulate are
     * currently unused, but since they have been in use please do not reuse them.
     *
     * #define XENMEM_access_op_enable_emulate     2
     * #define XENMEM_access_op_disable_emulate    3
     */
    #define XENMEM_access_op_set_access_multi   4

    typedef enum {
        XENMEM_access_n,
        XENMEM_access_r,
        XENMEM_access_w,
        XENMEM_access_rw,
        XENMEM_access_x,
        XENMEM_access_rx,
        XENMEM_access_wx,
        XENMEM_access_rwx,
        /*
         * Page starts off as r-x, but automatically
         * change to r-w on a write
         */
        XENMEM_access_rx2rw,
        /*
         * Log access: starts off as n, automatically
         * goes to rwx, generating an event without
         * pausing the vcpu
         */
        XENMEM_access_n2rwx,
        /* Take the domain default */
        XENMEM_access_default
    } xenmem_access_t;

    struct xen_mem_access_op {
        /* XENMEM_access_op_* */
        uint8_t op;
        /* xenmem_access_t */
        uint8_t access;
        domid_t domid;
        /*
         * Number of pages for set op (or size of pfn_list for
         * XENMEM_access_op_set_access_multi)
         * Ignored on setting default access and other ops
         */
        uint32_t nr;
        /*
         * First pfn for set op
         * pfn for get op
         * ~0ull is used to set and get the default access for pages
         */
        uint64_aligned_t pfn;
        /*
         * List of pfns to set access for
         * Used only with XENMEM_access_op_set_access_multi
         */
        XEN_GUEST_HANDLE(const_uint64) pfn_list;
        /*
         * Corresponding list of access settings for pfn_list
         * Used only with XENMEM_access_op_set_access_multi
         */
        XEN_GUEST_HANDLE(const_uint8) access_list;
    };
    typedef struct xen_mem_access_op xen_mem_access_op_t;
    DEFINE_XEN_GUEST_HANDLE(xen_mem_access_op_t);

    #define XENMEM_sharing_op                   22
    #define XENMEM_sharing_op_nominate_gfn      0
    #define XENMEM_sharing_op_nominate_gref     1
    #define XENMEM_sharing_op_share             2
    #define XENMEM_sharing_op_debug_gfn         3
    #define XENMEM_sharing_op_debug_mfn         4
    #define XENMEM_sharing_op_debug_gref        5
    #define XENMEM_sharing_op_add_physmap       6
    #define XENMEM_sharing_op_audit             7
    #define XENMEM_sharing_op_range_share       8

    #define XENMEM_SHARING_OP_S_HANDLE_INVALID  (-10)
    #define XENMEM_SHARING_OP_C_HANDLE_INVALID  (-9)

    /* The following allows sharing of grant refs. This is useful
     * for sharing utilities sitting as "filters" in IO backends
     * (e.g. memshr + blktap(2)). The IO backend is only exposed
     * to grant references, and this allows sharing of the grefs */
    #define XENMEM_SHARING_OP_FIELD_IS_GREF_FLAG   (xen_mk_ullong(1) << 62)

    #define XENMEM_SHARING_OP_FIELD_MAKE_GREF(field, val)  \
        (field) = (XENMEM_SHARING_OP_FIELD_IS_GREF_FLAG | val)
    #define XENMEM_SHARING_OP_FIELD_IS_GREF(field)         \
        ((field) & XENMEM_SHARING_OP_FIELD_IS_GREF_FLAG)
    #define XENMEM_SHARING_OP_FIELD_GET_GREF(field)        \
        ((field) & (~XENMEM_SHARING_OP_FIELD_IS_GREF_FLAG))

    struct xen_mem_sharing_op {
        uint8_t     op;     /* XENMEM_sharing_op_* */
        domid_t     domain;

        union {
            struct mem_sharing_op_nominate {  /* OP_NOMINATE_xxx           */
                union {
                    uint64_aligned_t gfn;     /* IN: gfn to nominate       */
                    uint32_t      grant_ref;  /* IN: grant ref to nominate */
                } u;
                uint64_aligned_t  handle;     /* OUT: the handle           */
            } nominate;
            struct mem_sharing_op_share {     /* OP_SHARE/ADD_PHYSMAP */
                uint64_aligned_t source_gfn;    /* IN: the gfn of the source page */
                uint64_aligned_t source_handle; /* IN: handle to the source page */
                uint64_aligned_t client_gfn;    /* IN: the client gfn */
                uint64_aligned_t client_handle; /* IN: handle to the client page */
                domid_t  client_domain; /* IN: the client domain id */
            } share;
            struct mem_sharing_op_range {         /* OP_RANGE_SHARE */
                uint64_aligned_t first_gfn;      /* IN: the first gfn */
                uint64_aligned_t last_gfn;       /* IN: the last gfn */
                uint64_aligned_t opaque;         /* Must be set to 0 */
                domid_t client_domain;           /* IN: the client domain id */
                uint16_t _pad[3];                /* Must be set to 0 */
            } range;
            struct mem_sharing_op_debug {     /* OP_DEBUG_xxx */
                union {
                    uint64_aligned_t gfn;      /* IN: gfn to debug          */
                    uint64_aligned_t mfn;      /* IN: mfn to debug          */
                    uint32_t gref;     /* IN: gref to debug         */
                } u;
            } debug;
        } u;
    };
    typedef struct xen_mem_sharing_op xen_mem_sharing_op_t;
    DEFINE_XEN_GUEST_HANDLE(xen_mem_sharing_op_t);

    /*
     * Attempt to stake a claim for a domain on a quantity of pages
     * of system RAM, but _not_ assign specific pageframes.  Only
     * arithmetic is performed so the hypercall is very fast and need
     * not be preemptible, thus sidestepping time-of-check-time-of-use
     * races for memory allocation.  Returns 0 if the hypervisor page
     * allocator has atomically and successfully claimed the requested
     * number of pages, else non-zero.
     *
     * Any domain may have only one active claim.  When sufficient memory
     * has been allocated to resolve the claim, the claim silently expires.
     * Claiming zero pages effectively resets any outstanding claim and
     * is always successful.
     *
     * Note that a valid claim may be staked even after memory has been
     * allocated for a domain.  In this case, the claim is not incremental,
     * i.e. if the domain's tot_pages is 3, and a claim is staked for 10,
     * only 7 additional pages are claimed.
     *
     * Caller must be privileged or the hypercall fails.
     */
    #define XENMEM_claim_pages                  24

    /*
     * XENMEM_claim_pages flags - the are no flags at this time.
     * The zero value is appropriate.
     */

    /*
     * With some legacy devices, certain guest-physical addresses cannot safely
     * be used for other purposes, e.g. to map guest RAM.  This hypercall
     * enumerates those regions so the toolstack can avoid using them.
     */
    #define XENMEM_reserved_device_memory_map   27
    struct xen_reserved_device_memory {
        xen_pfn_t start_pfn;
        xen_ulong_t nr_pages;
    };
    typedef struct xen_reserved_device_memory xen_reserved_device_memory_t;
    DEFINE_XEN_GUEST_HANDLE(xen_reserved_device_memory_t);

    struct xen_reserved_device_memory_map {
    #define XENMEM_RDM_ALL 1 /* Request all regions (ignore dev union). */
        /* IN */
        uint32_t flags;
        /*
         * IN/OUT
         *
         * Gets set to the required number of entries when too low,
         * signaled by error code -ERANGE.
         */
        unsigned int nr_entries;
        /* OUT */
        XEN_GUEST_HANDLE(xen_reserved_device_memory_t) buffer;
        /* IN */
        union {
            struct physdev_pci_device pci;
        } dev;
    };
    typedef struct xen_reserved_device_memory_map xen_reserved_device_memory_map_t;
    DEFINE_XEN_GUEST_HANDLE(xen_reserved_device_memory_map_t);

    #endif /* defined(__XEN__) || defined(__XEN_TOOLS__) */

    /*
     * XENMEM_get_vnumainfo used by guest to get
     * vNUMA topology from hypervisor.
     */
    #define XENMEM_get_vnumainfo                26

    /* vNUMA node memory ranges */
    struct xen_vmemrange {
        uint64_t start, end;
        unsigned int flags;
        unsigned int nid;
    };
    typedef struct xen_vmemrange xen_vmemrange_t;
    DEFINE_XEN_GUEST_HANDLE(xen_vmemrange_t);

    /*
     * vNUMA topology specifies vNUMA node number, distance table,
     * memory ranges and vcpu mapping provided for guests.
     * XENMEM_get_vnumainfo hypercall expects to see from guest
     * nr_vnodes, nr_vmemranges and nr_vcpus to indicate available memory.
     * After filling guests structures, nr_vnodes, nr_vmemranges and nr_vcpus
     * copied back to guest. Domain returns expected values of nr_vnodes,
     * nr_vmemranges and nr_vcpus to guest if the values where incorrect.
     */
    struct xen_vnuma_topology_info {
        /* IN */
        domid_t domid;
        uint16_t pad;
        /* IN/OUT */
        unsigned int nr_vnodes;
        unsigned int nr_vcpus;
        unsigned int nr_vmemranges;
        /* OUT */
        union {
            XEN_GUEST_HANDLE(uint) h;
            uint64_t pad;
        } vdistance;
        union {
            XEN_GUEST_HANDLE(uint) h;
            uint64_t pad;
        } vcpu_to_vnode;
        union {
            XEN_GUEST_HANDLE(xen_vmemrange_t) h;
            uint64_t pad;
        } vmemrange;
    };
    typedef struct xen_vnuma_topology_info xen_vnuma_topology_info_t;
    DEFINE_XEN_GUEST_HANDLE(xen_vnuma_topology_info_t);

    /* Next available subop number is 28 */

    #endif /* __XEN_PUBLIC_MEMORY_H__ */

    /*
     * Local variables:
     * mode: C
     * c-file-style: "BSD"
     * c-basic-offset: 4
     * tab-width: 4
     * indent-tabs-mode: nil
     * End:
     */